|  |
| --- |
| void setup() |
|  | { |
|  | pinMode(13, OUTPUT); //sets the digital pin as output |
|  | } |
|  |  |
|  | void loop() |
|  | { |
|  | digitalWrite(12,HIGH); //turns the LED on |
|  | delay(500); //waits for a second |
|  | digitalWrite(12,LOW); //turns the LED off |
|  | delay(500); //waits for a second |
|  | } |